Multihomed describes a computer [host](http://searchcio-midmarket.techtarget.com/definition/host) that has multiple [IP address](http://searchwindevelopment.techtarget.com/definition/IP-address)es to connected networks. A multihomed host is physically connected to multiple data links that can be on the same or different networks. For example, a computer with a Windows NT 4.0 Server and multiple IP addresses can be referred to as "multihomed" and may serve as an IP [router](http://searchnetworking.techtarget.com/definition/router).

A server can be multihomed which means it can have multiple internet interfaces or wireless interfaces and each of them can have different ip address

Python:

socket.bind(“0.0.0.0”,”8080”)

“0.0.0.0” means all interfaces